**Procurement of Medical Devices for the for the Institute for Cardiovascular Diseases „Dedinje“**

**IOP/21-2018/RD**

**Issued on October 29, 2018**

Question 1

In technical specification for id 1.4., under the point 9 is required bolus rate 0.2-1200 ml/h. Is it acceptable for the purchaser bolus in the range of 10-1200 ml/h, considering that in clinical practice bolus of 0.2 ml/h is not in usage, neither in pediatric practice.

Answer 1

Bolus flow rate of the range of 10 ml/h – 1200 ml/h is acceptable.