**Price Schedule - MRI Scanner**

**MRI System 1,5T with „Turnkey” site preparation**

|  |  |  |  |
| --- | --- | --- | --- |
| **Line Number** | **Specifications Required** | **Unit costs (DAP + unloaded)**  | **Currency****EUR/USD/RSD** |
| 1-8 | **MRI SYSTEM 1,5T** |  |  |
| 9 (I) | **ADDITIONAL EQUIPMENT (9.1+9.2+9.3+9.4+9.5)** |  |  |
| 9.1. | RF cabin for electromagnetic protection (damping value of min 90dB). RF cabin contains complete cabin with antistatic floor, door, window, antimagnetic lightening, all necessary filters, also with connections for gases supply of the anesthesia system, and all final works, for running requirements of MR scanner for work with the patients. |  |  |
| 9.2. | Chiller for MR gradient system cooling. |  |  |
| 9.3. | Electrical distribution cabinet for MR system. |  |  |
| 9.4. | Injector for MR studies. |  |  |
| 9.5. | Antimagnetic stretcher for patient transport. |  |  |
| 9 (II) | **WORKS AND SERVICES (9.6+9.7+9.8)** |  |  |
| 9.6 | Make location project based on space and room project where system will be installed. |  |  |
| 9.7 | Make project for civil, electro and thermo-technical works for technical room, examination room and control room. |  |  |
| 9.8 | Installation of the offered system- “Turnkey” project(Preparation of facilities- technical room, examination room and control room, HV cable from HV substation to technical room has to be provided by Beneficiaries).  |  |  |
| 10. | **TRAINING COSTS** |  |  |
|  | **CONTRACT PRICE (1-8+9 (I)+9(II)+10)** |  |  |